MC系列泵概述：

MC(U、R、H)系列产品是专门为输送磨机处理的矿物料而研发的悬臂式重型渣浆泵，特别适用于大颗粒、重磨蚀物料工况。被广泛用于冶金、矿山项目。该产品作为二相流输送浆体的底流泵，具有显著的经济价值。

MC Series Pumps Overview：

MC (U, R, H) series products are cantilever type heavy duty slurry pumps specially developed for conveying mineral materials handled by mills, especially suitable for large particles and heavy abrasive materials working conditions. It is widely used in metallurgy and mining projects. The product has significant economic value as a bottom flow pump for conveying slurry in two-phase flow.

MC泵特点：

* 大直径、低转速、高效率叶轮
* 最新耐磨材料
* 可互换的弹性体或金属内衬或全金属无内衬
* 简单的 "全面 "侧衬里调整
* 自定心填料箱设计
* 较大尺寸的过流件可快速进行“一体式”更换
* 可用的反向旋转提供了设备设计的灵活性

MC Pump Features:

* Large diameter, low speed, high efficiency impellers
* Latest wear resistant materials
* Interchangeable elastomer or metal liners, or unlined metal
* Simple “full face” side liner adjustment
* Self-centering stuffing box design
* Fast “one-piece” wet end changeout on larger sizes
* Available reverse rotations offer plant design flexibility

MC泵不同材料组合：

* MCR泵：橡胶护套，球磨铸铁泵体配套金属叶轮和金属/橡胶前护板和后护板
* MCU泵：全金属无内衬，硬质白口铸铁泵体配套金属叶轮、前护板和后护板
* MCM泵：硬质白口铸铁金属护套，球磨铸铁泵体配套金属叶轮、前护板和后护板

MC pumps in different material combinations:

* MCR pump: astomer liners inside ductile iron outer casing with metal impeller and metal or elastomer throatbush and frame plate liner insert
* MCU pump: all metal unlined hard white iron casing with metal impeller, throatbush and frame plate liner insert
* MCM pump: hard white iron metal liners inside ductile iron outer casing with metal impeller, throat bush and frame plate liner inser